[bookmark: _u01gx5vo3h3c]Vertical Ramp
[bookmark: _xno5zkerh6o2]Lacquered 6t Load
Vertical dock leveler with fixed lip (Alapont Global), dimensions 2200x1825mm with a 400mm lip. Manufactured with 5/7 teardrop pattern plate for the base and 13/15 teardrop pattern plate for the fixed lip. Standard dynamic capacity of 6,000 kg and static capacity of 9,000 kg. Fully anti-corrosion treated and powder-coated with polymerized paint, oven-cured at 200°C. Hydraulic power unit: 1.1 kW (1.5 HP), operating pressure 170 bar, with resistance to extreme temperatures (-20°C to +50°C). IP55 water-resistant electrical control panel equipped with an emergency stop button. Finish: RAL 9005 micro-textured black paint.
Vertical dock leveler with fixed lip (Alapont Global), dimensions 2200x2400mm with a 400mm lip. Manufactured with 5/7 teardrop pattern plate for the base and 13/15 teardrop pattern plate for the fixed lip. Standard dynamic capacity of 6,000 kg and static capacity of 9,000 kg. Fully anti-corrosion treated and powder-coated with polymerized paint, oven-cured at 200°C. Hydraulic power unit: 1.1 kW (1.5 HP), operating pressure 170 bar, with resistance to extreme temperatures (-20°C to +50°C). IP55 water-resistant electrical control panel equipped with an emergency stop button. Finish: RAL 9005 micro-textured black paint.
Vertical dock leveler with fixed lip (Alapont Global), dimensions 2200x2400mm with a 400mm lip. Manufactured with 5/7 teardrop pattern plate for the base and 13/15 teardrop pattern plate for the fixed lip. Standard dynamic capacity of 6,000 kg and static capacity of 9,000 kg. Fully anti-corrosion treated and powder-coated with polymerized paint, oven-cured at 200°C. Hydraulic power unit: 1.1 kW (1.5 HP), operating pressure 170 bar, with resistance to extreme temperatures (-20°C to +50°C). IP55 water-resistant electrical control panel equipped with an emergency stop button. Finish: RAL 9005 micro-textured black paint.

[bookmark: _xk0urqrkzlh9]Galvanized 6t
Vertical dock leveler with fixed lip (Alapont Global), dimensions 2200x1825mm with a 400mm lip. Manufactured with 5/7 teardrop pattern plate for the base and 13/15 teardrop pattern plate for the fixed lip. Standard dynamic capacity of 6,000 kg and static capacity of 9,000 kg. Fully anti-corrosion treated and powder-coated with polymerized paint, oven-cured at 200°C. Hydraulic power unit: 1.1 kW (1.5 HP), operating pressure 170 bar, with resistance to extreme temperatures (-20°C to +50°C). IP55 water-resistant electrical control panel equipped with an emergency stop button. Finish: Hot-dip galvanized.
Vertical dock leveler with fixed lip (Alapont Global), dimensions 2200x2400mm with a 400mm lip. Manufactured with 5/7 teardrop pattern plate for the base and 13/15 teardrop pattern plate for the fixed lip. Standard dynamic capacity of 6,000 kg and static capacity of 9,000 kg. Fully anti-corrosion treated and powder-coated with polymerized paint, oven-cured at 200°C. Hydraulic power unit: 1.1 kW (1.5 HP), operating pressure 170 bar, with resistance to extreme temperatures (-20°C to +50°C). IP55 water-resistant electrical control panel equipped with an emergency stop button. Finish: Hot-dip galvanized.
[bookmark: _548posyxahfv]Lacquered 15t Load
Vertical dock leveler with fixed lip (Alapont Global), dimensions 2200x1825mm with a 400mm lip. Manufactured with 5/7 teardrop pattern plate for the base and 13/15 teardrop pattern plate for the fixed lip. Standard dynamic capacity of 15,000 kg and static capacity of 18,000 kg. Fully anti-corrosion treated and powder-coated with polymerized paint, oven-cured at 200°C. Hydraulic power unit: 1.1 kW (1.5 HP), operating pressure 170 bar, with resistance to extreme temperatures (-20°C to +50°C). IP55 water-resistant electrical control panel equipped with an emergency stop button. Finish: RAL 9005 micro-textured black paint.
Vertical dock leveler with fixed lip (Alapont Global), dimensions 2200x2400mm with a 400mm lip. Manufactured with 5/7 teardrop pattern plate for the base and 13/15 teardrop pattern plate for the fixed lip. Standard dynamic capacity of 15,000 kg and static capacity of 18,000 kg. Fully anti-corrosion treated and powder-coated with polymerized paint, oven-cured at 200°C. Hydraulic power unit: 1.1 kW (1.5 HP), operating pressure 170 bar, with resistance to extreme temperatures (-20°C to +50°C). IP55 water-resistant electrical control panel equipped with an emergency stop button. Finish: RAL 9005 micro-textured black paint.

[bookmark: _4n0u7kk0t6f3]Galvanized 15t Load
Vertical dock leveler with fixed lip (Alapont Global), dimensions 2200x1825mm with a 400mm lip. Manufactured with 5/7 teardrop pattern plate for the base and 13/15 teardrop pattern plate for the fixed lip. Standard dynamic capacity of 15,000 kg and static capacity of 18,000 kg. Fully anti-corrosion treated and powder-coated with polymerized paint, oven-cured at 200°C. Hydraulic power unit: 1.1 kW (1.5 HP), operating pressure 170 bar, with resistance to extreme temperatures (-20°C to +50°C). IP55 water-resistant electrical control panel equipped with an emergency stop button. Finish: Hot-dip galvanized.
Vertical dock leveler with fixed lip (Alapont Global), dimensions 2200x2400mm with a 400mm lip. Manufactured with 5/7 teardrop pattern plate for the base and 13/15 teardrop pattern plate for the fixed lip. Standard dynamic capacity of 15,000 kg and static capacity of 18,000 kg. Fully anti-corrosion treated and powder-coated with polymerized paint, oven-cured at 200°C. Hydraulic power unit: 1.1 kW (1.5 HP), operating pressure 170 bar, with resistance to extreme temperatures (-20°C to +50°C). IP55 water-resistant electrical control panel equipped with an emergency stop button. Finish: Hot-dip galvanized.

