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Alapont Global protective bumpers, dimensions 125x575x105mm. Ensures safety and extends the lifespan of vehicles and equipment. Reinforced with 12mm steel for optimal performance. Cold-galvanised, anti-corrosive finish. Resistant to UV rays, acids and detergents. 

Alapont Global protective bumpers, measuring 250x440x90mm. Ensures safety and extends the lifespan of vehicles and equipment. Reinforced with 12mm steel for optimum performance. Anti-corrosive finish, cold-galvanised. Resistant to UV rays, acids and detergents. 

Alapont Global protective bumpers, measuring 540x250x105mm. Ensures safety and extends the lifespan of vehicles and equipment. Reinforced with 12mm steel for optimum performance. Anti-corrosive finish, cold-galvanised. Resistant to UV rays, acids and detergents. 

Movable protective bumpers
Alapont Global movable metal bumper, dimensions 500x250x110mm. Capable of vertical movement. Significantly reduces product wear by minimising friction with the vehicle. Made from 10 mm steel sheet, with 2 independent rubber bumpers. Compression spring for the buffer, ready for bolting or welding, with an anti-corrosion finish (cold-galvanised).

Rubber protective bumpers
Alapont Global rubber bumpers, dimensions 500x80x80mm. Highly durable, with a classic design, and most commonly used in basic standard installations. Suitable for both indoor and outdoor use; resistant to UV rays, acids and detergents. Anti-corrosive finish, cold-galvanised in black (RAL 9005).

Alapont Global rubber bumpers, measuring 250x250x100mm. Highly durable, with a classic design, and most commonly used in basic standard installations. Suitable for both indoor and outdoor use, resistant to UV rays, acids and detergents. Anti-corrosive finish, cold-galvanised in black RAL 9005.

Alapont Global rubber bumpers, measuring 500x250x90mm. Highly durable, with a classic design, and most commonly used in basic standard installations. Suitable for both indoor and outdoor use, resistant to UV rays, acids and detergents. Anti-corrosive finish, cold-galvanised in black RAL 9005.


