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Alapont Global hydraulic dock leveller with telescopic lip, dimensions 2000 x 2000mm with a 400mm lip, with a 5/7 mm tear-plate steel platform and lower structural reinforcements (10 IPN 100 type beams) to prevent deformation and a 13/15 mm lip. Standard dynamic capacity of 6,000 kg and static capacity of 9,000 kg. The lip is provided with 5º milling and folding that allows a smooth transition with the vehicle. Motor group of approx. 1.1 kW with resistance to extreme temperatures (-20°C to +50°C), anti-fall safety valves and smooth movements. Equipped with safety mast and side foot-guards. Micro-textured RAL 9005 black paint finish.
Alapont Global hydraulic dock leveller with telescopic lip, dimensions 2000 x 2300mm with a 400mm lip, with a 5/7 mm tear-plate steel platform and lower structural reinforcements (10 IPN 100 type beams) to prevent deformation and a 13/15 mm lip. Standard dynamic capacity of 6,000 kg and static capacity of 9,000 kg. The lip is provided with 5º milling and folding that allows a smooth transition with the vehicle. Motor group of approx. 1.1 kW with resistance to extreme temperatures (-20°C to +50°C), anti-fall safety valves and smooth movements. Equipped with safety mast and side foot-guards. Micro-textured RAL 9005 black paint finish.
Alapont Global hydraulic dock leveller with telescopic lip, dimensions 2000 x 2500mm with a 400mm lip, with a 5/7 mm tear-plate steel platform and lower structural reinforcements (10 IPN 100 type beams) to prevent deformation and a 13/15 mm lip. Standard dynamic capacity of 6,000 kg and static capacity of 9,000 kg. The lip is provided with 5º milling and folding that allows a smooth transition with the vehicle. Motor group of approx. 1.1 kW with resistance to extreme temperatures (-20°C to +50°C), anti-fall safety valves and smooth movements. Equipped with safety mast and side foot-guards. Micro-textured RAL 9005 black paint finish.
Alapont Global hydraulic dock leveller with telescopic lip, dimensions 2000 x 2800mm with a 400mm lip, with a 5/7 mm tear-plate steel platform and lower structural reinforcements (10 IPN 100 type beams) to prevent deformation and a 13/15 mm lip. Standard dynamic capacity of 6,000 kg and static capacity of 9,000 kg. The lip is provided with 5º milling and folding that allows a smooth transition with the vehicle. Motor group of approx. 1.1 kW with resistance to extreme temperatures (-20°C to +50°C), anti-fall safety valves and smooth movements. Equipped with safety mast and side foot-guards. Micro-textured RAL 9005 black paint finish.
Alapont Global hydraulic dock leveller with telescopic lip, dimensions 2000 x 3000mm with a 400mm lip, with a 5/7 mm tear-plate steel platform and lower structural reinforcements (10 IPN 100 type beams) to prevent deformation and a 13/15 mm lip. Standard dynamic capacity of 6,000 kg and static capacity of 9,000 kg. The lip is provided with 5º milling and folding that allows a smooth transition with the vehicle. Motor group of approx. 1.1 kW with resistance to extreme temperatures (-20°C to +50°C), anti-fall safety valves and smooth movements. Equipped with safety mast and side foot-guards. Micro-textured RAL 9005 black paint finish.
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Alapont Global hydraulic dock leveller with telescopic lip, dimensions 2000 x 2000mm with a 400mm lip, with a 5/7 mm tear-plate steel platform and lower structural reinforcements (10 IPN 100 type beams) to prevent deformation and a 13/15 mm lip. Standard dynamic capacity of 6,000 kg and static capacity of 9,000 kg. The lip is provided with 5º milling and folding that allows a smooth transition with the vehicle. Motor group of approx. 1.1 kW with resistance to extreme temperatures (-20°C to +50°C), anti-fall safety valves and smooth movements. Equipped with safety mast and side foot-guards. Hot-dip galvanized finish.
Alapont Global hydraulic dock leveller with telescopic lip, dimensions 2000 x 2300mm with a 400mm lip, with a 5/7 mm tear-plate steel platform and lower structural reinforcements (10 IPN 100 type beams) to prevent deformation and a 13/15 mm lip. Standard dynamic capacity of 6,000 kg and static capacity of 9,000 kg. The lip is provided with 5º milling and folding that allows a smooth transition with the vehicle. Motor group of approx. 1.1 kW with resistance to extreme temperatures (-20°C to +50°C), anti-fall safety valves and smooth movements. Equipped with safety mast and side foot-guards. Hot-dip galvanized finish.
Alapont Global hydraulic dock leveller with telescopic lip, dimensions 2000 x 2500mm with a 400mm lip, with a 5/7 mm tear-plate steel platform and lower structural reinforcements (10 IPN 100 type beams) to prevent deformation and a 13/15 mm lip. Standard dynamic capacity of 6,000 kg and static capacity of 9,000 kg. The lip is provided with 5º milling and folding that allows a smooth transition with the vehicle. Motor group of approx. 1.1 kW with resistance to extreme temperatures (-20°C to +50°C), anti-fall safety valves and smooth movements. Equipped with safety mast and side foot-guards. Hot-dip galvanized finish.
Alapont Global hydraulic dock leveller with telescopic lip, dimensions 2000 x 2800mm with a 400mm lip, with a 5/7 mm tear-plate steel platform and lower structural reinforcements (10 IPN 100 type beams) to prevent deformation and a 13/15 mm lip. Standard dynamic capacity of 6,000 kg and static capacity of 9,000 kg. The lip is provided with 5º milling and folding that allows a smooth transition with the vehicle. Motor group of approx. 1.1 kW with resistance to extreme temperatures (-20°C to +50°C), anti-fall safety valves and smooth movements. Equipped with safety mast and side foot-guards. Hot-dip galvanized finish.
Alapont Global hydraulic dock leveller with telescopic lip, dimensions 2000 x 3000mm with a 400mm lip, with a 5/7 mm tear-plate steel platform and lower structural reinforcements (10 IPN 100 type beams) to prevent deformation and a 13/15 mm lip. Standard dynamic capacity of 6,000 kg and static capacity of 9,000 kg. The lip is provided with 5º milling and folding that allows a smooth transition with the vehicle. Motor group of approx. 1.1 kW with resistance to extreme temperatures (-20°C to +50°C), anti-fall safety valves and smooth movements. Equipped with safety mast and side foot-guards. Hot-dip galvanized finish.
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Alapont Global hydraulic dock leveller with telescopic lip, dimensions 2000 x 2000mm with a 400mm lip, with a 5/7 mm tear-plate steel platform and lower structural reinforcements (10 IPN 100 type beams) to prevent deformation and a 13/15 mm lip. Standard dynamic capacity of 15,000 kg and static capacity of 18,000 kg. The lip is provided with 5º milling and folding that allows a smooth transition with the vehicle. Motor group of approx. 1.1 kW with resistance to extreme temperatures (-20°C to +50°C), anti-fall safety valves and smooth movements. Equipped with safety mast and side foot-guards. Hot-dip galvanized finish.
Alapont Global hydraulic dock leveller with telescopic lip, dimensions 2000 x 2300mm with a 400mm lip, with a 5/7 mm tear-plate steel platform and lower structural reinforcements (10 IPN 100 type beams) to prevent deformation and a 13/15 mm lip. Standard dynamic capacity of 15,000 kg and static capacity of 18,000 kg. The lip is provided with 5º milling and folding that allows a smooth transition with the vehicle. Motor group of approx. 1.1 kW with resistance to extreme temperatures (-20°C to +50°C), anti-fall safety valves and smooth movements. Equipped with safety mast and side foot-guards. Hot-dip galvanized finish.
Alapont Global hydraulic dock leveller with telescopic lip, dimensions 2000 x 2500mm with a 400mm lip, with a 5/7 mm tear-plate steel platform and lower structural reinforcements (10 IPN 100 type beams) to prevent deformation and a 13/15 mm lip. Standard dynamic capacity of 15,000 kg and static capacity of 18,000 kg. The lip is provided with 5º milling and folding that allows a smooth transition with the vehicle. Motor group of approx. 1.1 kW with resistance to extreme temperatures (-20°C to +50°C), anti-fall safety valves and smooth movements. Equipped with safety mast and side foot-guards. Hot-dip galvanized finish.
Alapont Global hydraulic dock leveller with telescopic lip, dimensions 2000 x 2800mm with a 400mm lip, with a 5/7 mm tear-plate steel platform and lower structural reinforcements (10 IPN 100 type beams) to prevent deformation and a 13/15 mm lip. Standard dynamic capacity of 15,000 kg and static capacity of 18,000 kg. The lip is provided with 5º milling and folding that allows a smooth transition with the vehicle. Motor group of approx. 1.1 kW with resistance to extreme temperatures (-20°C to +50°C), anti-fall safety valves and smooth movements. Equipped with safety mast and side foot-guards. Hot-dip galvanized finish.
Alapont Global hydraulic dock leveller with telescopic lip, dimensions 2000 x 3000mm with a 400mm lip, with a 5/7 mm tear-plate steel platform and lower structural reinforcements (10 IPN 100 type beams) to prevent deformation and a 13/15 mm lip. Standard dynamic capacity of 15,000 kg and static capacity of 18,000 kg. The lip is provided with 5º milling and folding that allows a smooth transition with the vehicle. Motor group of approx. 1.1 kW with resistance to extreme temperatures (-20°C to +50°C), anti-fall safety valves and smooth movements. Equipped with safety mast and side foot-guards. Hot-dip galvanized finish.
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Alapont Global hydraulic dock leveller with telescopic lip, dimensions 2000 x 2000mm with a 400mm lip, with a 5/7 mm tear-plate steel platform and lower structural reinforcements (10 IPN 100 type beams) to prevent deformation and a 13/15 mm lip. Standard dynamic capacity of 15,000 kg and static capacity of 18,000 kg. The lip is provided with 5º milling and folding that allows a smooth transition with the vehicle. Motor group of approx. 1.1 kW with resistance to extreme temperatures (-20°C to +50°C), anti-fall safety valves and smooth movements. Equipped with safety mast and side foot-guards. Micro-textured RAL 9005 black paint finish.
Alapont Global hydraulic dock leveller with telescopic lip, dimensions 2000 x 2300mm with a 400mm lip, with a 5/7 mm tear-plate steel platform and lower structural reinforcements (10 IPN 100 type beams) to prevent deformation and a 13/15 mm lip. Standard dynamic capacity of 15,000 kg and static capacity of 18,000 kg. The lip is provided with 5º milling and folding that allows a smooth transition with the vehicle. Motor group of approx. 1.1 kW with resistance to extreme temperatures (-20°C to +50°C), anti-fall safety valves and smooth movements. Equipped with safety mast and side foot-guards. Micro-textured RAL 9005 black paint finish.
Alapont Global hydraulic dock leveller with telescopic lip, dimensions 2000 x 2500mm with a 400mm lip, with a 5/7 mm tear-plate steel platform and lower structural reinforcements (10 IPN 100 type beams) to prevent deformation and a 13/15 mm lip. Standard dynamic capacity of 15,000 kg and static capacity of 18,000 kg. The lip is provided with 5º milling and folding that allows a smooth transition with the vehicle. Motor group of approx. 1.1 kW with resistance to extreme temperatures (-20°C to +50°C), anti-fall safety valves and smooth movements. Equipped with safety mast and side foot-guards. Micro-textured RAL 9005 black paint finish.
Alapont Global hydraulic dock leveller with telescopic lip, dimensions 2000 x 2800mm with a 400mm lip, with a 5/7 mm tear-plate steel platform and lower structural reinforcements (10 IPN 100 type beams) to prevent deformation and a 13/15 mm lip. Standard dynamic capacity of 15,000 kg and static capacity of 18,000 kg. The lip is provided with 5º milling and folding that allows a smooth transition with the vehicle. Motor group of approx. 1.1 kW with resistance to extreme temperatures (-20°C to +50°C), anti-fall safety valves and smooth movements. Equipped with safety mast and side foot-guards. Micro-textured RAL 9005 black paint finish.
Alapont Global hydraulic dock leveller with telescopic lip, dimensions 2000 x 3000mm with a 400mm lip, with a 5/7 mm tear-plate steel platform and lower structural reinforcements (10 IPN 100 type beams) to prevent deformation and a 13/15 mm lip. Standard dynamic capacity of 15,000 kg and static capacity of 18,000 kg. The lip is provided with 5º milling and folding that allows a smooth transition with the vehicle. Motor group of approx. 1.1 kW with resistance to extreme temperatures (-20°C to +50°C), anti-fall safety valves and smooth movements. Equipped with safety mast and side foot-guards. Micro-textured RAL 9005 black paint finish.


